# Completion aid

The red parts must be overwritten by the project proponent.

The *red parts in italics* give an explanation of what the project proponent has to provide at this place.

The black parts are default entries, which will apply to most projects. The project proponent is free to change them, but must use the track-change-mode if doing so.

**Project Design Document**

Logo of the project to be inserted here

Name of project: xxx

Name of quality manager: xxx

Date of issue: xx.xx.xxxx

Methodology: EBC-Guidelines for the Certification of Biochar Based Carbon Sinks Version 2.1

Project location: xxx

Project start date: XX.XX.XXXX *(Date of contract conclusion with Carbon Standards or registration date for the EBC Biochar C-Sink service. Or, in the case of retroactive certification, the production date of the batch.)*

Project period: The project has no end date, but it is verified on an annual basis

Project summary: *(2 sentences about the project)*

The project will increase carbon sequestration by working the produced biochar into different matrixes and in this way create a long-term carbon storage with a persistence of up to 100 years as according to the EBC Biochar C-Sink Standard. Without the project, no C-sink would be created since *feedstock* does not constitute a long-term carbon reservoir.

In the initial 5 years of the project we expect carbon sequestration of approximately xxx CO2eq in total or xxx CO2eq / year.

**Table of content**

[Completion aid 1](#_Toc161145604)

[1. Purpose and general description of project 5](#_Toc161145605)

[1.1. Project location 5](#_Toc161145606)

[1.2. Description of baseline scenario 5](#_Toc161145607)

[1.3. Biochar carbon sinks 5](#_Toc161145608)

[1.4. Project Boundary 5](#_Toc161145609)

[1.5. Eligibility 6](#_Toc161145610)

[1.6. Additionality 6](#_Toc161145611)

[1.6.1. Assessment of regulatory requirements for biochar production and application as a removal technology 6](#_Toc161145612)

[1.6.2. Assessment of contribution of Biochar C-sink credits to biochar and/or biomass price. 6](#_Toc161145613)

[1.6.3. Assessment of additionality test according to the CDM Tool for additionality 6](#_Toc161145614)

[2. Ex-ante estimate of impact 6](#_Toc161145615)

[3. Technology and business cases 7](#_Toc161145616)

[3.1. Production unit 7](#_Toc161145617)

[3.2. Feedstock 7](#_Toc161145618)

[3.3. Distribution channels of biochar 8](#_Toc161145619)

[3.4. Planned business development 9](#_Toc161145620)

[4. Determination of C-sink potential 9](#_Toc161145621)

[4.1. Monitoring plan 9](#_Toc161145622)

[4.1.1. General data 9](#_Toc161145623)

[4.1.2. Emissions from fossil fuels 10](#_Toc161145624)

[4.1.3. Methane emissions 12](#_Toc161145625)

[4.2. Calculation of C-sink potential at factory gate 13](#_Toc161145626)

[4.2.1. Emissions from fossil fuels 13](#_Toc161145627)

[4.2.2. Methane emissions 16](#_Toc161145628)

[4.2.3. Value of C-sink potential 17](#_Toc161145629)

[5. Determination of C-sink 18](#_Toc161145630)

[5.1. Biochar processing 18](#_Toc161145631)

[5.1.1. Monitoring of processing parameters 18](#_Toc161145632)

[5.1.2. Calculation of processing emissions 18](#_Toc161145633)

[5.2. Registration of C-sink 19](#_Toc161145634)

[5.2.1. Monitoring of transport parameters until final location 19](#_Toc161145635)

[5.2.2. Calculation of C -sink 20](#_Toc161145636)

[5.2.3. Geological C-sink 20](#_Toc161145637)

[6. Annexes 20](#_Toc161145638)

# Purpose and general description of project

The project *(projectname)* compromises xx pyrolysis plants for biochar production from *(feedstock).* Biochar is a hyper versatile material with an increasing number of applications in agriculture, environmental engineering, and basic industry. Biochar applied a matrix permitted by the Global C-Sink Standard poses a stable carbon sink (C-sink). Without the project, no C-sink would be created since Pomace does not constitute a long-term carbon reservoir.

*(Write about 2 sentences about baseline.)*

Another objective of the project is to improve the soil quality in xx by marketing biochar as soil amendment. Biochar can improve soil quality significantly because of its impact on the soil pH, its water retention capacity, and its ability to store nutrients.

Furthermore, the biochar may be used as temporary C-sink or as additive in construction materials or consumer products.

## Project location

*(Where will the project take place?)*

*(Provide GPS location of pyrolysis unit)*

The geographical locations of the subsequently installed plants will be documented in the biochar tool *(or other dMRV tool*).

*(Where will biochar sold to)*

*(Provide map indicating the before mentioned regions)*

## Description of baseline scenario

*(Describe Baseline)*

The baseline scenario for carbon removal accounting is the "business as usual", in which no permanent biochar-based carbon sink is generated and is considered as zero. The fact that biomass could have been used differently in the baseline scenario, has no impact on the consideration of the baseline as zero.

## Biochar carbon sinks

When plant biomass is burnt or decomposed, the assimilated carbon is released again in the form of CO2. However, if the plant biomass is pyrolyzed, about half of the plant carbon is transformed into a mixture of predominantly very persistent carbon compounds that form a solid material known as biochar. While in the environment, any carbon compound is subject to degradation; for most components of biochar, this process is extremely slow, and mostly even so slow, that it is hard to measure for thousands of years. Provided that the biochar is not burned, the biochar carbon remains as a C-sink in the terrestrial system.

## Project Boundary

Scope 1 and Scope 2 emissions as well as transport emissions from Scope 3 in connection with the production, processing and application of biochar for the creation of a C-sink.

## Eligibility

*(All checkmarks have to be ticked)*

□ Production of biochar according to EBC/WBC criteria in place.

□ Producer is a legal entity and hold an operating license for the entire project region.

□ Social Impact: The project complies with the requirements set by the methodology, see annex 17-0-2EN Self-Assessment Social Responsibility.

## Additionality

The required additionality test on project level follows a 3 step approach. If combinations of 1.6.1 and 1.6.2, or 1.6.1 and 1.6.3 can be positively answered, the project is additional.

## Assessment of regulatory requirements for biochar production and application as a removal technology

*(Assess whether biochar production and carbon preserving application is required in the country where the producer operates. All relevant permits and regulations need to be presented. A project is only additional, if no legally binding requirements for the production and carbon-preserving application of biochar can be identified.)*

## Assessment of contribution of Biochar C-sink credits to biochar and/or biomass price.

*(Evidence of the contribution of the sales of the C-sink credits to reducing the price of the biochar and/or the acquired biomass must be presented. A “significant contribution” of the selling price of the C-sink credits to the affordability of biochar shall be proven.)*

## Assessment of additionality test according to the CDM Tool for additionality

*(In case 1.6.2 cannot be applied, the Clean Development Mechanism (CDM) Tool for the demonstration and assessment of additionality shall be applied in its most recent version. In this tool, either an investment analysis or a barrier analysis can be applied.*

*For the investment analysis, the “benchmark analysis” shall be conducted, as there are other revenue streams than the revenue from the C-sink credits.*

*The common practice analysis can be skipped.)*

# Ex-ante estimate of impact

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Year of operation | Amount of feedstock (DM) | C-sink potential (tCO2eq) | Established temporary C-sinks (tC) | Established permanent C-sinks (tCO2eq) |
| 1 | X | X | X | X |
| 2 | X | X | X | X |
| 3 | X | X | X | X |
| 4 | X | X | X | X |
| 5 | X | X | X | X |
| sum | X | X | X | X |

# Technology and business cases

## Production unit

Biochar is produced via pyrolysis technology. Pyrolysis means the thermo-chemical decomposition of the feedstock under the exclusion of oxygen.

By converting sustainable biomass into biochar by pyrolysis, a long-term carbon reservoir is created. At the factory gate of the production unit the biochar poses a potential of C-sink (C-sink potential). It could still be burned. By safety measures, such as marketing and labeling the biochar with the aim of becoming ana C-sink and monitoring all distribution channels in a digital Measurement, Reporting and Verification tool (dMRV), it is ensured in the best possible way, that the biochar is used to form a C-sink. C-sink certificates are only issued for those parts of the biochar for which it can be proven that they have been put in a matrix. Without the project, no C-sink would be created, as non-pyrolytic biomass does not ensure persistent carbon storage.

The produced biochar is certified under the xx Biochar Certification (xBC) standard, what guarantees that the biomass feedstock is sustainably procured and produced, biochar fulfils the analytical threshold values so no damage is caused to the environment, emissions limits of the pyrolysis unit are adhered to and storage procedures are environmentally sound.

The biochar production follows the xx Biochar Certification (xBC) standard, which ensures:

* Compliance with laws regarding air pollution control
* Minimization of risks on human health, social and environmental impacts
* Energy and carbon efficiency
* Sustainable origin of the feedstock

Type of pyrolysis unit

Xxx,

Planned operating hours per year: xx

Planned feedstock consumption: xx

Nominal biochar production: xx

Concept for waste energy and/or carbon recovery

*(Provide details on how you plan energy recovery, concerning energy and technical implementation. )*

*(provide company flowchart from technical pre-audit)*

## Feedstock

All used feedstock corresponds to the EBC positive list.

Only C-neutral biomass input materials are permitted for the production of biochar C-sinks. Biochar produced from biomass whose harvesting resulted in the destruction or depletion of a natural C-sink (e.g., clear-cutting of a forest) or has contributed to the disappearance of an existing sink (e.g., inappropriate agricultural practices on bog soil) does not render any positive climate service and must not be used for C-sink-potential certification.

However, it must be ensured that the removal of harvest residues does not decrease soil organic carbon stocks .

In the project the following feedstock is used which is eligible with the sustainability criteria:

|  |
| --- |
| xxxx |

Origin of feedstock:

*(Describe what feedstock the producer is using and how it was used before the biochar production started.)*

The feedstock mentioned above corresponds to the general feedstock classes:

□ (1) Agricultural biomasses

□ (2) Organic residues from food processing

□ (3) Wood from landscape conservation, short rotation plantations, arable forestry, forest gardens, field margins, and urban areas

□ (4) Biomass from forest management

□ (5) Wood waste

□ (6) Other biogenic residues

To avoid methane emissions during storage of biomass the following principles should be followed:

*(Producers can also get a custom storage plan approved by Carbon Standards.)*

* Wood and other biomass should be chipped only a few days and at a maximum of four weeks before pyrolysis. Log storage is considered unproblematic regarding methane emissions; coarse wood (thinner logs, branches, cuttings, etc.) should be stored as airy as possible and not mixed with green waste.
* If just-in-time chipping is not possible, the wood chips or biomass should be dried as soon as possible, e.g., with the excess heat from pyrolysis and stored dry with a maximum of 20% residual moisture. If the biomass is sufficiently dry, biodegradation does not take place or is slowed down considerably.
* Alternatively, the wood chips or the biomasses can be stored in small, well-ventilated containers such as lattice boxes (max. 2 m3). Due to sufficient ventilation, anaerobic degradation and thus methane emissions can be prevented.

If compliance with these principles cannot be fulfilled, actual practice and parameters according to the monitoring plan will be documented.

## Distribution channels of biochar

The following applications are possible for this project:

* Geological C-sink (biochar applied to soil)

*(If other applications are planned please name them and amend section 5 accordingly.)*

## Planned business development

*Describe producers plans for business development. E.g. feedstock usage, distribution channels, scale-up.*

# Determination of C-sink potential

## Monitoring plan

All data which are required to calculate the C-sink potential is entered into a dMRV System. The dMRV system is either provided by Carbon Standards or by an external MRV systemprovider. External MRV systems and tools must be endorsed by Carbon Standards annually. The data will be monitored as mentioned below. Each packaging unit containing more than 1 m3 of biochar must be labeled with a scannable identification code provided by the biochar dMRV System, which shows the following information:

- Date of production

- EBC certification class

- Feedstock used

- Highest pyrolysis temperature

- Bulk density

- Biochar properties as per lab analysis

- Indication whether C-sink value has already been sold elsewhere on the packaging and the delivery bill by stating if the C-sink value of the biochar has already been compensated.

Packaging units smaller than 1 m3 biochar may be grouped into a larger unit (e.g., 20 bags of 50 l packed on a palette) where the larger unit is labeled with the scannable identification code, given that all smaller units have the same destination.

### General data

The following general data will be monitored:

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Monitoring frequency** | **Source of data** |
| Batch Start Date | per batch | Internal documentation |
| Batch End Date | per batch | Internal documentation |
| H/Corg ratio | per batch | laboratories endorsed by Carbon Standards, see <https://www.carbon-standards.com/en/standards/service-501~ebc-c-sink.html> section Laboratories |
| C-content of biochar | per batch | laboratory endorsed by Carbon Standards, see <https://www.carbon-standards.com/en/standards/service-501~ebc-c-sink.html> section Laboratories |
| M\_biochar (DM)  (Total biochar production of batch (expected) in t dry matter) | Per batch | Protocols documenting the sampling.  Dry weight and total carbon content per big bag is recorded by means of drying a sample of biochar all 10 m3, according to methods explained in EBC Biochar C-sink Standard, chapter 5.1. |
| Biochar Production (DM) | continous | operation recordings |

The following general conversion rates are fixed ex-ante:

*(If project proponent wants to use different parameters they have to be well justified and accepted by Carbon Standards.)*

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Ex-ante definition; value** | **Source of data** |
| CO2 emissions from diesel | 3.2 kg CO2eq / kg diesel or 2.7 kg CO2eq / l diesel | Methodology, Juhrich, 2016 |
| CO2 emissions from heavy fuel | 65 t CO2eq / TJ | Methodology, Juhrich, 2016 |

### Emissions from fossil fuels

#### Feedstock

For the feedstock the following parameters will be monitored:

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Monitoring frequency** | **Source of data** |
| Type of feedstock (with ID of EBC positive list) | continuous | purchase receipts and EBC positive list |
| Average water content of feedstock at delivery | per batch | documentation of frequent measurements |
| Amount of feedstock (DM) processed for the last batch | per batch | production protocols |
| Total amount of feedstock (dry matter) used for the batch | per batch | production planning |
| Amount of fertilizers used as per the following table in kg N | for each feedstock delivery | x |
| Area on that pesticides were used as per the following table in ha | for each feedstock delivery | x |
| Amount of input of fuels for cultivation and harvest | for each feedstock delivery | x |
| Amount of diesel used for feedstock preparation | continuous | purchase receipts |
| Amount of electricity used for feedstock preparation | continuous | electricity meter |
| CO₂eq of electricity used for the pyrolysis plant in g CO₂eq/kWh | per batch | electricity provider |
| How do you dry the feedstock? | continuous | Statement |
| Amount of fuel equivalent used for drying per ton (DM) of feedstock? | continuous | purchase receipts |
| Amount of electric energy used for drying per ton (DM) of feedstock | continuous | purchase receipts |

The following general conversion rates are fixed ex-ante:

*(If project proponent wants to use different parameters they have to be well justified and accepted by Carbon Standards.)*

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Ex-ante definition; value** | **Source of data** |
| CO2 emissions from Nitrogen fertilizer | 1 t CO2eq / 100 kg N | Methodology, Zhang et al., 2013 |
| CO2 emissions from pesticides | 94 kg CO2eq per hectare | Methodology, Audsley et al., 2009 |

#### Pyrolysis

For pyrolysis the following parameters will be monitored:

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Monitoring frequency** | **Source of data** |
| Electricity consumption of pyrolyser for the entire batch (in kWh) | per batch | x |
| Source of electric energy for the pyrolysis plant | per batch | x |
| CO₂eq footprint of electricity used for the pyrolysis plant in g CO₂eq/kWh | per batch | electricity provider |
| Energy source to preheat the pyrolysis reactor | per batch | x |
| Amount of fuel which is used to preheat the pyrolysis reactor in t per batch | per batch | x |
| CO₂eq of fuel used for the pyrolysis plant per t | per batch | invoices for purchasing fossil fuels |

If it is assumed that the carbon yield in the biochar is less than 10% of the carbon contained in the biomass the biochar C-sink may be established using the pro rata approach*. If you are holding an exception permit regarding pro rata approach, please provide the additional data you monitor.*

#### Post-treatment

For post-treatment of the biochar the following parameters will be monitored:

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Monitoring frequency** | **Source of data** |
| Amount of diesel used for biochar post-treatment | per batch | purchase receipts |
| Amount of electricity used for biochar post-treatment | per batch | purchase receipts |

#### Compensation of Fossil Emissions

Emissions resulting from the provision of biomass (fuel consumption, N2O from fertilizer) affect the carbon footprint and are compensated by deductions in the C-sink calculation.

### Methane emissions

#### Storage of biomass

When biomass is stored, methane emissions can be produced, which need to be included in the C-sink potential calculation. This is why the storage period needs to be monitored. Not only the storage on the premises of the pyrolysis plant is considered, but the entire storage period of the biomass, be it at the harvest site or the site of any biomass processor or trader.

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Monitoring frequency** | **Source of data** |
|  | continuous | operation recordings |
| A) Is storage duration less than a month? Yes/No | continuous | operation recordings |
| If Answer to A) is no:  B) Is biomass stored well ventilated? Yes/No | continuous | operation recordings |
| If Answer to B) is no:  C) Is moisture content below 20%? Yes/No | continuous | operation recordings |
| core temperature of the biomass for all sites where biomass is stored for more than one month | annually | measurement during on-site inspection |

If at least one Point A) to C) is answered with yes: methane emissions are negligible.

If all points A) to C) are answered with no or temperatures of more than 5°C above ambient temperature is measured during on-site inspection: methane emissions are included in the C-sink potential calculation.

#### Pyrolysis

During pyrolysis, the pyrolysis gases are usually oxidized in a suitably designed combustion chamber. Usually, the gaseous combustion products pass a filtration step and are then emitted mostly as CO2. If the pyrolysis process is well-adjusted and the combustion chamber correctly designed, non-CO2 GHGs and other pollutants can be kept at very low levels in the exhaust. However, CH4, NOx, CO, and particulate matter (PM) are, as in all combustion processes, never completely absent and must be controlled. Concerning the net climate impact, methane emission is particularly important to measure. CO, NOx, SOx, and PM are also harmful to the environment, but according to the IPCC, they do not have a clear greenhouse gas effect (IPCC, 2013) and are therefore not accounted for the emission portfolio, while CH4 is included.

Measuring methane emissions below 5 ppm is technically complex. Continuous measurement over an entire production year is not possible with currently available technology. Therefore, either at least two CH4-emission tests per pyrolysis unit with the same feedstock representing the typical operation of the unit are required, or the pyrolysis unit must have a system certification according to EBC or WBC.

The average methane emission of a type of system is then set to be the mean value plus one standard deviation. If an emission measurement for methane or CxHx is below the measuring accuracy of the instruments, the limit of quantification (LOQ) is used. The assessed methane emissions are thus higher than the calculated average and provide a sufficiently high safety margin to cover any potential emission peaks, e.g., during start-up and shutdown of operation.

|  |  |
| --- | --- |
| □ | Default: Pyrolysis unit used in the project has a system certification, see system certification. |
| xxx |

Accordingly, ex-ante definition of the following parameter:

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Ex-ante definition; value** | **Source of data** |
| [CH4\_emissions\_pyrolysis] | xxx | system certification |

|  |  |
| --- | --- |
| □ | Pyrolysis unit used in the project has no system certification. A detailed measurement strategy with precise details of the measurement technology, measurement intervals, and measurement for CH4 emission tests will be provided to Carbon Standards and approved.  *Provision of details on testing strategy required.* |

Accordingly, following parameter will be monitored once during first monitoring period:

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Monitoring frequency** | **Source of data** |
| [CH4\_emissions\_pyrolysis] in kg CH4/t DM feedstock | At least 2 measurements during first monitoring period | measurements |

#### Compensation of CH4 Emissions

Methane emissions can be compensated with short-term C-sinks, provided they guarantee at least 20 years of carbon storage.

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Monitoring frequency** | **Source of data** |
| Proof of compensation | per batch | xx |

## Calculation of C-sink potential at factory gate

The C-sink potential at factory gate reflects the remaining C-content of the biochar at factory gate, for which all fossil emissions have been offset against a permanent sink. Preferably the permanent portion of the biochar itself.

### Emissions from fossil fuels

Emissions from fossil fuels are calculated based on the following formulas:

#### Feedstock

The production of biomass usually causes emissions that need to be accounted for as carbon expenditures of the C-sink. Emissions are calculated in t CO2eq.

* If mineral nitrogen fertilization was used to produce the biomass, its carbon footprint, including soil borne N2O emissions, must be accounted for according to the formula 100 kg N = 1 t CO2eq (Zhang et al., 2013). This represents a consideration of the GWP100 for N2O and the production emissions for nitrogen fertilizer.
* If pesticides were used, a flat value of 94 kg CO2eq per hectare (Audsley et al., 2009) is applied for their production-related emissions.
* The input of fuels for cultivation and harvest or preparation of feedstock must also be added to the emission portfolio with a conversion factor of 3.2 kg CO2eq / kg diesel or 2.7 kg CO2eq / l diesel (Juhrich, 2016).
* The fuel for trucks for transporting the biomass from the source to the biochar production facility must be calculated with the conversion factor of 2.7 kg CO2eq per liter diesel and the road distance according to google maps. If the truck returns back empty, the distance will be multiplied by 2.
* Emissions for drying feedstock are calculated, fuel and electricity are considered. The fuel for drying feedstock is calculated with a conversion factor of 2.7 kg CO2eq per liter diesel.

The total biomass related GHG emissions without Methane per batch is calculated according to the following formula:

#### Pyrolysis

Emissions which are produced during the pyrolysis process contain electricity consumption and fuel for preheating the pyrolysis reactor. The emissions are calculated in **tCO2eq.**

Note: If renewable energy is used, a CO2eq footprint of zero is assumed. If the pyrolysis plant itself generates at least as much electricity on an annual average as is consumed in the production facility, a CO2eq of zero is assumed for electricity consumption.

The total production emissions are calculated with the formula:

*If you are holding an exception permit regarding pro rata approach please provide the formulas how to calculate .*

#### Post-treatment

If the biochar will be post-treated, the emissions are calculated according to the following formula:

#### Leakage emissions

The Global C-Sink Standard prohibits non-sustainable biomass cultivation, land use change and soil organic carbon depletion - thus, leakage in sense of carbon expenditure outside of the project boundaries is avoided as much as possible. It is assumed that activity shifts to biochar production causes only minimal leakage emissions.

For the EBC Biochar C-Sink, the emissions from Scope 1 and 2 are fully recorded. As per project boundary, from Scope 3, only the emissions from biomass production and its transport are directly quantified. Other indirect emissions from Scope 3 are not recorded individually due to their comparatively low volume but are instead included in the calculation with a flat margin of safety.

This includes, for example, the emissions caused by:

- Production and disposal of polypropylene bags,

- Electricity for the operation and cooling of the company's external computer servers,

- Potential methane emissions during the first month of storage of the biomass,

- Fuel consumption by employees for commuting to work and for business trips,

- Marketing and management activities including trade shows and conference attendance,

- Operation of chainsaws or harvesters for felling and peeling trees and for digging up roots,

- Emissions from machine fuels during cultivation of agricultural land and plant protection measures,

- Production, maintenance, repair, and disposal of pyrolysis equipment, transport vehicles, warehouses, and other machinery.

- The margin further contains unavoidable imprecisions of the C-sink accounting such as sampling, packaging, volume and dry mater analysis, etc.

- Unlikely loss of c-sink material e.g. by burning small portions of diffuse C-sinks in waste incineration plants

The margin of safety generally to 10% of the total emissions from biochar production deducted from the C-sink value and is rounded to 0.1%.

### Methane emissions

During biomass storage and pyrolysis process methane emissions are produced. They are calculated according to the following formula:

#### Emissions from the storage of the biomass

If methane emissions are negligible according to section 3.1.3.1.: 0 tCH4

If methane emissions are included in the C-sink potential calculation: Emissions are calculated in **tCH4**:

Default values given in the methodology are used:

|  |  |
| --- | --- |
|  | 0,15% of C-content for woody biomass  0,25% of C-content for non-woody biomass |
|  | 48% for woody biomass 50% for non-woody biomass |

#### CH4 Emissions from Pyrolysis reactor

Emissions are calculated in **tCH4.**

*Adjustment may be needed.*

#### Compensation of CH4 Emissions

The greenhouse gas emissions caused by biochar production, quantified from planting the biomass to the packaging of the biochar, are then converted from CO2eq into the rate of carbon expenditure (= CO2eq / 44u \* 12u) per ton of biochar. This carbon expenditure rate is then subtracted from the carbon content of the biochar, which results in the value of the C-sink of the biochar at the factory gate.

With GWP20\_CH4 = 86 CO2eq

The methane emissions can be compensated with short-term C-sinks, provided they guarantee at least 20 years of carbon storage.

### Value of C-sink potential

The C-sink potential at factory gate reflects the remaining C-content of the biochar at factory gate.

# Determination of C-sink

Once the C-sink potential of the biochar has been determined and the label has been applied to the packaging units in accordance with the requirements in chapter 3.1, the further fate of the biochar is only indirectly influenced by the producer. In the further chain up to the final C-sink, there are processors and users. It is incumbent on all of them to play their part in quality assurance and monitoring as well as reporting on their emissions. The final C-sink is registered by the first C-sink owner.

## Biochar processing

If the biochar is delivered to a processing company who makes new biochar-based products from the biochar, the receiving company must be EBC or WBC certified as a processing company and/or trader. This allows the verification of the climate relevant processes as part of annual on-site inspection. All processing steps must be recorded with their CO2eq footprint.

Once the products are repackaged, they must be registered as new product and C-sink unit providing the following information:

- Product processor

- Biochar production batch ID and/or QR code to access EBC/WBC biochar analysis.

- Date of biochar production

- Point of new departure (GPS)

- Biochar C-content of product

- C-sink matrix, if mixed to one

- Emission that occurred during processing

- Indication whether C-sink value has already been sold elsewhere on the packaging and the delivery bill by stating if the C-sink value of the biochar has already been compensated.

### Monitoring of processing parameters

Processors are obliged to monitor the following data:

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Monitoring frequency** | **Source of data** |
| Amount of diesel used for transportation | continuous | distance and amount of trucks |
| Amount of diesel used for biochar processing | continuous | operation recordings |
| Amount of electricity used for biochar processing | continuous | operation recordings |
| Input biochar and output biochar based-product documentation | continuous | operation recordings |
| Any other GHG emitting process | continuous | operation recordings |

### Calculation of processing emissions

The calculation of the processing emissions is done with the following formula:

# Registration of C-sink

Biochar carbon sinks must be registered with the geo-localized area where the biochar or its derived products have been applied. This encompasses scenarios where biochar serves as a soil amendment or finds application in various contexts, such as construction for residential, infrastructural, or road-related purposes.

If the registration of the geographical location and site owner of the C-sink is not possible or practicable, but the biochar is nevertheless shown to have been introduced into a matrix that precludes combustion (e.g., compost, biogas slurry, cement, etc., see above), the sink is considered a diffuse C-sink.

The following information are registered for biochar carbon sink:

* C-sink owner (e.g. owner of the land where the C-sink is established, owner of the material that contains the biochar, producer of biochar containing products).
* KLM-file of land or area where the C-sink was established.
* Date of C-sink establishment.
* EBC/WBC batch number.
* Biochar analysis
* Type of C-sink (geo-localized or diffuse).
* C-sink matrix.
* Amount of biochar in dry tons.
* Amount of carbon in CO2eq.
* C-sink project design document
* Validation report of the validation body
* Verification report of the verification body
* Monitoring report of the operation

### Monitoring of transport parameters until final location

First C-sink owners are obliged to monitor the following data:

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Monitoring frequency** | **Source of data** |
| Amount of diesel used for transportation from last processor to application site | continuous | Distance and amount of trucks; in case of diffuse C-sink: statistically determined mean distance |
| Amount of diesel used for application | continuous | operation recordings |
| Any other GHG emitting process | continuous | operation recordings |
| Emission reports from Producer and Processors | per C-sink | Producer and Processors |

### Calculation of C -sink

The C-sink is registered in the Global C-sink Registry.

If H/Corg ratio is < 0,4, the calculation of the C-sink at day of application is :

*If the biochar used has a H/Corg ratio > 0,4 individual process of offsetting emissions must be described.*

However, every biochar C-sink underlies a time-dependent evolution, and the C-sink is a measure of the mass of carbon that is physically present in the C-sink matrix at any given moment in time since the establishment of the C-sink. The size of a biochar C-sink is, thus, a function of the type of biochar determining its specific persistence in a specific C-sink matrix and the time since the application to the C-sink matrix.

### Geological C-sink

Biochar which is applied to soil can be registered as geological C-sink if the biochar has an H/Corg ratio < 0.4.

A conservative average degradation rate of 0.3% per year may be assumed for higher temperature biochars with a H : Corg ratio below 0.4 (following: Budai et al., 2013; Camps-Arbestain et al., 2015).

Thus, 100 years after soil application, 74% of the original carbon in biochar could still be accounted for as sequestered carbon. The annual rate of 0.3% is based on the most conservative metanalytical estimate for biochar carbon degradation published to date.

*Provide details if biochar is used other than soil application.*

# Annexes

1. Social Responsibility